[DB]
host=local.beijingyongan.com
user=ya
password=ya@2017
dbname=yaxt
encoding=gb2312
port=9702
usedb=0

[SERVER_SETTING]
;websocket_url=ws://localhost:8086/
tcp_host=0.0.0.0
tcp_port=9700
websocket_url=ws://192.168.1.115:8086/
;websocket_url=ws://124.204.33.42:8086/
interval_send_json_postion=1000
interval_send_json_counting=10000
interval_send_json_alarm=10000
interval_send_json_device=5000
interval_send_json_drivingface=30000
interval_send_json_leader=1800000
interval_load_leader=14400000
<<<<<<< HEAD
ws_connect_inteval=6000
send_call_interval=5000
=======
cal_vehicle_meeting=5000
send_call_interval=3000
>>>>>>> newprotocal
send_help_interval=5000
heart_interval=5000
locate_type=0
websocket_url_bk=
use_filter=1
recon_server=0
recon_db=0
reader_lost=0
card_lost=0
timing_interval=0
sampling_interval=2000
z_offset=0.000000
coor_error=0.000000
ranging_error=0.000000
moving_error=0.000000

[TESTTOOL]
write_log=0
show_data=1
vehicle_title_count=12
reader_title_count=7
reader_synctime_count=11
card_tdoa_count=13
card_adhoc_count=6
light_title_count=8

[TESTTOOL_PAGE]
page_reader=1
page_reader_max_rows=4000
page_card_tof=0
page_card_tof_max_rows=4000
page_card_tdoa=1
page_card_tdoa_max_rows=4000
page_synctime=1
page_synctime_max_rows=4000
page_card_adhoc=0
page_card_adhoc_max_rows=4000

[TESTTOOL_VEHICLE_COLUMN_0]
col_title=序号
col_width=60
col_field=DESC
col_visible=1

[TESTTOOL_VEHICLE_COLUMN_1]
col_title=卡号
col_width=80
col_field=card_id
col_visible=1
[TESTTOOL_VEHICLE_COLUMN_2]
col_title=分站
col_width=40
col_field=reader_id
col_visible=1
[TESTTOOL_VEHICLE_COLUMN_3]
col_title=天线
col_width=40
col_field=antenna_id
col_visible=0
[TESTTOOL_VEHICLE_COLUMN_4]
col_title=分站时间
col_width=60
col_field=reader_stamp
col_visible=1
[TESTTOOL_VEHICLE_COLUMN_5]
col_title=卡时间
col_width=60
col_field=card_stamp
col_visible=1
[TESTTOOL_VEHICLE_COLUMN_6]
col_title=飞行时间
col_width=60
col_field=fly_time
col_visible=1
[TESTTOOL_VEHICLE_COLUMN_7]
col_title=距离(m)
col_width=80
col_field=distance
col_visible=1
[TESTTOOL_VEHICLE_COLUMN_8]
col_title=定位方法
col_width=60
col_field=ranging_type
col_visible=1
[TESTTOOL_VEHICLE_COLUMN_9]
col_title=电量
col_width=40
col_field=power
col_visible=1
[TESTTOOL_VEHICLE_COLUMN_10]
col_title=加速度
col_width=60
col_field=acceleration
col_visible=1
[TESTTOOL_VEHICLE_COLUMN_11]
col_title=接收时间
col_width=150
col_field=rec_time
col_visible=1

[TESTTOOL_READER_COLUMN_0]
col_title=序号
col_width=60
col_field=DESC
col_visible=1
[TESTTOOL_READER_COLUMN_1]
col_title=分站号
col_width=60
col_field=reader_id
col_visible=1
[TESTTOOL_READER_COLUMN_2]
col_title=分站IP
col_width=120
col_field=reader_ip
col_visible=1
[TESTTOOL_READER_COLUMN_3]
col_title=分站时间戳
col_width=80
col_field=reader_stamp
col_visible=1
[TESTTOOL_READER_COLUMN_4]
col_title=状态
col_width=60
col_field=reader_state
col_visible=1
[TESTTOOL_READER_COLUMN_5]
col_title=接收时间
col_width=150
col_field=rec_time
col_visible=1
[TESTTOOL_READER_COLUMN_6]
col_title=分站时间
col_width=150
col_field=reader_time
col_visible=1

[TESTTOOL_SYNCTIME_COLUMN_0]
col_title=序号
col_width=60
col_field=DESC
col_visible=1
[TESTTOOL_SYNCTIME_COLUMN_1]
col_title=本地分站
col_width=60
col_field=local_reader
col_visible=1
[TESTTOOL_SYNCTIME_COLUMN_2]
col_title=本地天线
col_width=60
col_field=local_antenna
col_visible=1
[TESTTOOL_SYNCTIME_COLUMN_3]
col_title=上级分站
col_width=60
col_field=upper_reader
col_visible=1
[TESTTOOL_SYNCTIME_COLUMN_4]
col_title=上级天线
col_width=60
col_field=upper_antenna
col_visible=1
[TESTTOOL_SYNCTIME_COLUMN_5]
col_title=同步序号
col_width=60
col_field=sync_num
col_visible=1
[TESTTOOL_SYNCTIME_COLUMN_6]
col_title=同步等级
col_width=60
col_field=reader_level
col_visible=1
[TESTTOOL_SYNCTIME_COLUMN_7]
col_title=本地发送时间
col_width=150
col_field=send_time
col_visible=1
[TESTTOOL_SYNCTIME_COLUMN_8]
col_title=接收上级时间
col_width=150
col_field=upper_time
col_visible=1
[TESTTOOL_SYNCTIME_COLUMN_9]
col_title=ROOT分站
col_width=150
col_field=root_reader
col_visible=1
[TESTTOOL_SYNCTIME_COLUMN_10]
col_title=ROOT天线
col_width=150
col_field=root_antenna
col_visible=1

[TESTTOOL_TDOA_COLUMN_0]
col_title=序号
col_width=60
col_field=DESC
col_visible=1
[TESTTOOL_TDOA_COLUMN_1]
col_title=卡号
col_width=80
col_field=card_id
col_visible=1
[TESTTOOL_TDOA_COLUMN_2]
col_title=分站
col_width=40
col_field=reader_id
col_visible=1
[TESTTOOL_TDOA_COLUMN_3]
col_title=天线
col_width=40
col_field=antenna_id
col_visible=0
[TESTTOOL_TDOA_COLUMN_4]
col_title=分站时间戳
col_width=60
col_field=reader_stamp
col_visible=1
[TESTTOOL_TDOA_COLUMN_5]
col_title=卡时间戳
col_width=60
col_field=card_stamp
col_visible=1
[TESTTOOL_TDOA_COLUMN_6]
col_title=TDOA时间
col_width=150
col_field=fly_time
col_visible=1
[TESTTOOL_TDOA_COLUMN_7]
col_title=分站同步序号
col_width=60
col_field=sync_num
col_visible=1
[TESTTOOL_TDOA_COLUMN_8]
col_title=定位方法
col_width=60
col_field=ranging_type
col_visible=1
[TESTTOOL_TDOA_COLUMN_9]
col_title=电量
col_width=40
col_field=power
col_visible=1
[TESTTOOL_TDOA_COLUMN_10]
col_title=加速度
col_width=60
col_field=acceleration
col_visible=1
[TESTTOOL_TDOA_COLUMN_11]
col_title=卡类型
col_width=50
col_field=card_type
col_visible=1
[TESTTOOL_TDOA_COLUMN_12]
col_title=信号强度
col_width=60
col_field=strength
col_visible=1
[TESTTOOL_TDOA_COLUMN_13]
col_title=X轴加速度
col_width=60
col_field=acc1
col_visible=1
[TESTTOOL_TDOA_COLUMN_14]
col_title=Y轴加速度
col_width=60
col_field=acc2
col_visible=1
[TESTTOOL_TDOA_COLUMN_15]
col_title=Z轴加速度
col_width=60
col_field=acc3
col_visible=1

[TESTTOOL_ADHOC_COLUMN_0]
col_title=序号
col_width=60
col_field=DESC
col_visible=1
[TESTTOOL_ADHOC_COLUMN_1]
col_title=源地址
col_width=60
col_field=card_id
col_visible=1
[TESTTOOL_ADHOC_COLUMN_2]
col_title=命令字
col_width=60
col_field=cmd
col_visible=1
[TESTTOOL_ADHOC_COLUMN_3]
col_title=时间戳
col_width=60
col_field=timestamp
col_visible=1
[TESTTOOL_ADHOC_COLUMN_4]
col_title=节点级别
col_width=60
col_field=level
col_visible=1
[TESTTOOL_ADHOC_COLUMN_5]
col_title=接收时间
col_width=120
col_field=rec_time
col_visible=1

[TESTTOOL_LIGHT_COLUMN_0]
col_title=序号
col_width=60
col_field=DESC
col_visible=1
[TESTTOOL_LIGHT_COLUMN_1]
col_title=灯号
col_width=60
col_field=light_id
col_visible=1
[TESTTOOL_LIGHT_COLUMN_2]
col_title=地址
col_width=60
col_field=addr
col_visible=1
[TESTTOOL_LIGHT_COLUMN_3]
col_title=命令字
col_width=60
col_field=cmd
col_visible=1
[TESTTOOL_LIGHT_COLUMN_4]
col_title=颜色
col_width=60
col_field=color
col_visible=1
[TESTTOOL_LIGHT_COLUMN_5]
col_title=形状
col_width=60
col_field=shape
col_visible=1
[TESTTOOL_LIGHT_COLUMN_6]
col_title=控制分站
col_width=60
col_field=ctrl_reader_id
col_visible=1
[TESTTOOL_LIGHT_COLUMN_7]
col_title=接收时间
col_width=120
col_field=rec_time
col_visible=1

[MONITOR]
server_handle=2756940
server_path=C:\dev_projects\yong_an\src\yaserver\..\..\output\Debug\bin\YAServer.exe
is_default=1
is_master=0
heart_interval=15
server_interval=12
server_local=-1062731773
server_remote=-1062731764
heart_local=167772161
heart_remote=167772162
monitor_handle=1706530
monitor_path=E:\git\YASolution\src\win32\..\..\output\Debug\bin\YAMonitor.exe
sel_net={7F2753AC-3CAA-4484-B729-8BED4A56C43E}


[READER_SET]
interval_time=200

[SERVER_LOG]
system_status=1
raw_data=1	
parse_data=1
send_event=1
rev_event=1
locate_data=1
